**Hardware implementation**

The hardware implementation of our embedded position tracking system is straightforward. Teensy-3.6 development board (Teensy) and TCD1304 linear CCD (Toshiba) are the two major components. Besides, it also requires some simple resistance, capacitance, etc. to robustly drive the image sensor. The detailed diagram is shown below.

